**DRAINAGE CB AND INLET NOTES**

***Unless Otherwise Noted***

1. Catch basin connections and inlet connections must be 8" diameter. Pipe must be cement mortar lined ductile iron Class 50 (MIN) per Specification 9-05.3. Fittings must be cement mortar lined ductile iron. Joints must be rubber gasket, push-on or mechanical.
2. Bedding must be Class D with select native material.
3. Catch basin connections must be placed at a minimum slope of 2% and a maximum slope of 100% per Standard Plan No. 261 and Specification 7-08.3(4).
4. Inlet connections must be placed at a minimum slope of 5% and a maximum slope of 50% per Specification 7-08.3(5).
5. Catch basins and inlets must be located per Standard Plan No. 260a and 260b.
6. Television inspection of catch basin connections must be per Specification 7-17.3(3)G.
7. Contractors are not allowed to core into mains or structures without prior approval from SPU. To schedule core taps, contact SPU at 206-615-0511 a minimum of 2 business days in advance. SPU shall be on site prior to the start of contractor performed core tap. Contractors performing core taps must provide the coupon of removed material to SPU.