**RAIN GARDEN NOTES**

***Unless Otherwise Noted***

1. Rain garden grading and bottom area shall be as shown on the approved plan. Subgrade shall be scarified 4 inches minimum. Soil shall be compost amended for 12 inches minimum or 12 inches minimum of bioretention soil shall be placed. Imported bioretention soil, if used, shall be per Specification 9-14.1(3).
2. If shown on the approved plan, berm material shall be the same as rain garden soil mounded a minimum of 2 inches above finished grade and compacted to 90% dry density.
3. Arborist wood mulch shall be per Specification 9-14.4(4). Finished grade shall be one inch below walks and curbs.
4. Rain garden landscaping shall be as shown on the approved plan. Changes to the approved landscaping plan require submittal of a revised landscaping plan.
5. After planting, rain gardens shall be inspected and approved by the City of Seattle, or an approved representative.
6. Protect all rain gardens from accumulating sediments and compaction. Any impacted rain garden shall be restored to fully functioning condition by removal of sediment laden soils, over excavation as approved the City of Seattle, or an approved representative and replacement with new bioretention soil per Specification 9-14.1(3).
7. Water to ensure vegetation survival.